Pinguino IDE Installation & Use Instructions
*************************************************

Pinguino was written in 2008 by Jean-Pierre Mandon and released under a GPL license.
Since its initial release there have been numerous bug fixes and improvements.
As of February 2010, the code was moved to Google Code where all the "users turned developers"
can access the same source tree.
Pinguino is constantly being updated with all the users' and developers' input.

This file is free documentation; you have unlimited permission to copy, 
distribute and modify it.

Pinguino is an arduino like environment built in Python.
It is a complete package with compiler, assembler, linker and bootloader.
Pinguino is compatible with arduino/wiring langage.

dependencies:

Linux
- libusb
- python 2.5
- wxpython 2.8

Windows
- python 2.5
- wxpython 2.8

Mac OS X 10.6 (Snow Leopard)
- python 2.6.1 (32 bit)
- wxpython 2.8 (32 bit)
- libusb 0.1.4
- pyusb 0.4.3

Pinguino (8 bit) is based on open source software:
- compiler			SDCC 		http://sdcc.sourceforge.net/
- asm/linker		GPUTILS		http://gputils.sourceforge.net/
- bootloader (v1,2)	VASCO project	http://vasco.gforge.enseeiht.fr/
- bootloader (v3)	Diolan		http://www.diolan.com/pic/
- bootloader (v4)	JAL Project	http://www.justanotherlanguage.org/
					and Alexander Enzmann's USB Framework
- IDE				Python		http://www.python.org/

Pinguino (32 bit) is based on open source software:
- compiler		GCC		http://http://gcc.gnu.org/
- asm/linker	BINUTILS	http://www.gnu.org/
- C library		Newlib		http://sourceware.org/newlib/
- IDE			Python		http://www.python.org/
			
Contributions, bug reports and questions are welcome.
rblanchot@gmail.com
yeison.eng@gmail.com
