*** Pinguino EasyPack for win32, release note ***

First, to extract 7z archive , '7-Zip' has to be installed from here,
     http://www.7-zip.org/

Installation and start up Pinguno IDE:
  1. Using 7-Zip, extract 'Pinguino-X4-EasyPack-Win32-RevNNN-vNN-yyyy-mm.7z' to the arbitrary folder.
     (N,y,m is number or string) 
     It's highly recommended extracting this archive file to the folder 
     which name dose not have 'spaces or multibyte strings'.
  2. Move the x4-easy-revNNN folder to i.e. 'C:\x4-easy-revNNN'.
     (Because gpasm.exe can't recognize the long folder name.) 
  3. Execute x4-easy-revNNN\pinguino.exe,
     or
     x4-easy-revNNN\pinguino_start.bat

THAT'S ALL!!

But... :D
Prerequisite:
  1. If you encounter the message of not existing 'msvc*90.dll' in Windows,
     it has to be installed from here:
       vcredist_x86.exe (for win32),
         http://www.microsoft.com/en-us/download/details.aspx?id=5582&WT.mc_id=MSCOM_EN_US_DLC_DETAILS_131Z4ENUS22004
     or as Python v2.6.6 includes 'msvc*90.dll' file , you may install the Python instead of vcredist_x86.exe
       form here,
         http://www.python.org/ftp/python/2.6.6/python-2.6.6.msi
  2. On 8bit PICs, if you encounter the error message of "sdcpp can't find ..." during compilation,  
     add SDCC execution path to Windows environment variable PATH.
     i.e.
	 If you extract EasyPack to c:\x4-easy-revNNN (NNN is revision number),
	 add  c:\x4-easy-revNNN\win32\p8\bin to Windows environment variable PATH.
	 
	 General information about PATH setting: [ http://www.computerhope.com/issues/ch000549.htm ]

Note:
* This package dose not install the device drivers,
  they have to be installed according to the instruction below link,
  Windows XP:
     http://wiki.pinguino.cc/index.php/Windows#Pinguino_Driver
  Windows 7
     http://wiki.pinguino.cc/index.php/Windows_7
* If Pinguino IDE dosn't start well, delete '.config' file and restart Pinguino IDE,
  or check 'pinguino.log' or 'pingunoPanic' file in Pinguino root folder.
  
Tested environment:
  * This package has been tested only 'win32' environment at this moment,
    Windows XP (on VMWare),
    Windows 7(32bit).


This package based on:
  Pinguino: http://pinguino.cc 
      [ svn checkout http://pinguino32.googlecode.com/svn/ide/ pinguino32 ]
  Python: v2.6.6    
      [ http://www.python.org/ftp/python/2.6.6/python-2.6.6.msi ]
  Py2exe: v0.6.9
      [ http://sourceforge.net/projects/py2exe/files/py2exe/0.6.9/py2exe-0.6.9.win32-py2.6.exe/download ]
  PySerial: v2.5
      [ http://sourceforge.net/projects/pyserial/files/pyserial/2.5/pyserial-2.5.win32.exe/download ]
  pyusb-1.0.0a2-py2.6:
      [ http://sourceforge.net/projects/pyusb/files/PyUSB%201.0/1.0.0-alpha-2/pyusb-1.0.0a2.zip/download ]
  wxPython: 2.8.12.1(unicode) for Python 2.6
      [ http://downloads.sourceforge.net/wxpython/wxPython2.8-win32-unicode-2.8.12.1-py26.exe ]
   msvcp90.dll: (Using Ver.9.00.30729.1)
      This file will be found in c:\Windows\winsxs or so on.
Memo:
  PySVN(not inclueded):  v1.7.6
    http://pysvn.tigris.org/files/documents/1233/49192/py26-pysvn-svn173-1.7.6-1457.exe

Packaging scripts and patches:
  Refer to 'extra/EasyPack-doc' folder.






Thank you very much, Pinguino Developper Team, many committers 
and community members.


History:
rev999    v01: 2014/04, packaged and released by avrin.
rev996    v01: 2014/04, packaged and released by avrin.
rev903    v01: 2013/10, packaged and released by avrin.
rev857    v01: 2013/05, packaged and released by avrin.
rev685mod v01: 2013/02, packaged and released by avrin.

2014/04: by avrin

